IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Description: "Option [Drawing Scale: 100.000000]"
Description: "Option [Global Unique Identifiers (GUID): Keep existing]"
Description: "Option [Elements to export: Visible elements (on all stories)]"
Description: "Option [Partial Structure Display: Entire Model]"
Description: "Option [IFC Domain: All]"
Description: "Option [Structural Function: All Elements]"
Description: "Option [Convert Grid elements: On]"
Description: "Option [Convert IFC Annotations and ArchiCAD 2D elements: Off]"
Description: "Option [Convert 2D symbols of Doors and Windows: Off]"
Description: "Option [Explode Composite and Complex Profile elements into parts: Off]"
Description: "Option [Export geometries that Participates in Collision Detection only: On]"
Description: "Option [Multi-skin complex geometries: Building element parts]"
Description: "Option [Elements in Solid Element Operations: Extruded/revolved]"
Description: "Option [Elements with junctions: Extruded/revolved without junctions]"
Description: "Option [Slabs with slanted edge(s): Extruded]"
File name: "C:\Users\CTP1\Documents\2402-03_VALENTIN\2402-03_PRO---VALENTIN\2024-1213_PRO-3D_2402-03_VALENTIN.ifc"
Time stamp: "2024-12-13T10:20:44"
Author: "Architect"
Organization: "Building Designer Office"
Preprocessor: "PreProc - EDM 5.0"
Originating system: "IFC file generated by Graphisoft ArchiCAD-64 18.0.0 FRA FULL Windows version (IFC2x3 add-on version: 3006 FRA FULL)."
Authorization: "The authorising person"
Application: "ArchiCAD-64" version "18.0.0" identifier "IFC2x3 add-on version: 3006 FRA FULL" by Organization "Graphisoft" id "GS" description "Graphisoft"

People and organizations
  Person "Non défini" of Organization "Non défini"
  Owner history of Person "Non défini" of Organization "Non défini" | application "ArchiCAD-64" version "18.0.0" identifier "IFC2x3 add-on version: 3006 FRA FULL" by Organization "Graphisoft" id "GS" description "Graphisoft" | change ADDED | created 1734081642 (2024-12-13T09:20:42Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  SOLIDANGLEUNIT: STERADIAN
  CURRENCY: EUR
  TIMEUNIT: Year (conversion based)
  MASSUNIT: GRAM
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  LUMINOUSINTENSITYUNIT: LUMEN

Spatial structure
IFCPROJECT "Projet"
  IFCSITE "Site" | latitude 48° 52′ 0″ | longitude 2° 20′ 0″ | elevation above sea level 0.
    IFCBUILDING "Bâtiment"
      IFCBUILDINGSTOREY "FOND / 79.00 ngf" | elevation -1950.
        contains 7 elements
          5 x IFCSLAB | type IFCSLABTYPE "15 % 196800 600" | FLOOR | names: "Dalle-034" | material: layers "15 % 196800 600" ("15 % 196800" 600.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "25 % 2670121569 D50" | object type "25 % 2670121569 D50" | names: "Pot-040" | material: "25 % 2670121569" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCSLAB | type IFCSLABTYPE "75 % 2669794085 1380" | ROOF | names: "Toit-24" | material: layers "75 % 2669794085 1379.79" ("75 % 2669794085" 1379.78981932) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
      IFCBUILDINGSTOREY "TOPO / 79.95 ngf" | elevation -1000.
        contains 77 elements
          44 x IFCCOLUMN | type IFCCOLUMNTYPE "25 % 2670121569 D30" | object type "25 % 2670121569 D30" | names: "Pot-029", "Pot-030" | material: "25 % 2670121569" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          7 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "75 % 2034597177 300" | names: "Mur-089", "Mur-092", "Mur-093" (+1 more) | material: layers "75 % 2034597177 300" ("75 % 2034597177" 300.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "15 % 196800 200" | names: "Mur-082" | material: layers "15 % 196800 200" ("15 % 196800" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "HACHURE MANQUANTE 269029580 450" | names: "Mur-082", "Mur-084", "Mur-085" (+2 more) | material: layers "HACHURE MANQUANTE 269029580 450" ("HACHURE MANQUANTE 269029580" 450.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "75 % 2034597177 270" | names: "Mur-090", "Mur-089" | material: layers "75 % 2034597177 270" ("75 % 2034597177" 270.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCSTAIR | names: "Esc-034" | material: "50 %" | property sets: AC_Pset_RenovationAndPhasing, Pset_StairCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "75 % 2034597177 200" | names: "Mur-091", "Mur-093", "Mur-092" | material: layers "75 % 2034597177 200" ("75 % 2034597177" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "75 % 2669925280 200" | names: "Mur-082" | material: layers "75 % 2669925280 200" ("75 % 2669925280" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre 18" | names: "Fen-092" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "25 % 2670121569 D200" | object type "25 % 2670121569 D200" | names: "Pot-033" | material: "25 % 2670121569" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
      IFCBUILDINGSTOREY "RDC / 81.41 ngf" | elevation 460.
        contains 50 elements
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Tube rampe 18" | names: "MOB-0066" | material: "Sans Trame" | property sets: AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "75 % 2669925280 100" | names: "Mur-094", "Mur-095" | material: layers "75 % 2669925280 100" ("75 % 2669925280" 100.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "100 % 2668484876 80" | names: "Mur-093" | material: layers "100 % 2668484876 80" ("100 % 2668484876" 80.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          8 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 150" | names: "Mur-093", "Mur-094" | material: layers "0 - HACHURE ISOLANT 309885812 150" ("0 - HACHURE ISOLANT 309885812" 150.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre 18" | names: "Fen-092" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre 18" | names: "Fen-092", "Fen-094" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "100 % 2668484876 200" | names: "Mur-094" | material: layers "100 % 2668484876 200" ("100 % 2668484876" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCSLAB | type IFCSLABTYPE "15 % 196800 230" | FLOOR | names: "Dalle-028" | material: layers "15 % 196800 230" ("15 % 196800" 230.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          9 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "15 % 196800 200" | names: "Mur-086", "Mur-085" | material: layers "15 % 196800 200" ("15 % 196800" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCSLAB | type IFCSLABTYPE "100 % 2668484876 70" | FLOOR | names: "Dalle-028" | material: layers "100 % 2668484876 70" ("100 % 2668484876" 70.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCCOLUMN | type IFCCOLUMNTYPE "25 % 2670121569 D200" | object type "25 % 2670121569 D200" | names: "Pot-033" | material: "25 % 2670121569" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Bois 45 2682958634 200 x 200" | object type "Bois 45 2682958634 200 x 200" | names: "Pou-034" | material: "Bois 45 2682958634" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 20" | names: "Mur-093", "Mur-095" | material: layers "0 - HACHURE ISOLANT 309885812 20" ("0 - HACHURE ISOLANT 309885812" 20.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCSTAIR | names: "Esc-029" | material: "50 %" | property sets: AC_Pset_RenovationAndPhasing, Pset_StairCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "100 % 2668484876 340" | names: "Mur-094" | material: layers "100 % 2668484876 340" ("100 % 2668484876" 340.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre 18" | names: "Fen-094" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCBEAM | type IFCBEAMTYPE "Bois 45 2682958634 200 x 520" | object type "Bois 45 2682958634 200 x 520" | names: "Pou-034" | material: "Bois 45 2682958634" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          1 x IFCSLAB | type IFCSLABTYPE "15 % 196800 40" | FLOOR | names: "Dalle-029" | material: layers "15 % 196800 40" ("15 % 196800" 40.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "100 % 2668484876 503" | FLOOR | names: "Dalle-030" | material: layers "100 % 2668484876 502.5" ("100 % 2668484876" 502.5) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "100 % 2668484876 930" | FLOOR | names: "Dalle-028" | material: layers "100 % 2668484876 930" ("100 % 2668484876" 930.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "100 % 2668484876 645" | FLOOR | names: "Dalle-029" | material: layers "100 % 2668484876 645" ("100 % 2668484876" 645.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "100 % 2668484876 788" | FLOOR | names: "Dalle-028" | material: layers "100 % 2668484876 787.5" ("100 % 2668484876" 787.5) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "100 % 2668484876 20" | names: "Mur-093" | material: layers "100 % 2668484876 20" ("100 % 2668484876" 20.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 60" | names: "Mur-093" | material: layers "0 - HACHURE ISOLANT 309885812 60" ("0 - HACHURE ISOLANT 309885812" 60.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
      IFCBUILDINGSTOREY "R+1 / 84.25 ngf" | elevation 3960.
        contains 48 elements
          2 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Poutre acier universel 18" | names: "MOB-0066" | material: "Sans Trame" | property sets: AC_Pset_RenovationAndPhasing
          3 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Cadre main cour 18" | names: "MOB-0062" | material: "Sans Trame" | property sets: AC_Pset_RenovationAndPhasing
          10 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 150" | names: "Mur-093", "Mur-094", "Mur-082" (+1 more) | material: layers "0 - HACHURE ISOLANT 309885812 150" ("0 - HACHURE ISOLANT 309885812" 150.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "100 % 859257570 200" | names: "Mur-082" | material: layers "100 % 859257570 200" ("100 % 859257570" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          3 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "15 % 196800 200" | names: "Mur-085", "Mur-093" | material: layers "15 % 196800 200" ("15 % 196800" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          3 x IFCWINDOW | type IFCWINDOWSTYLE "Ouverture fenêtre rectangulaire 18" | names: "Fen-093", "Fen-094" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, AC_Pset_RenovationAndPhasing
          4 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "75 % 2669794085 100" | names: "Mur-082", "Mur-094", "Mur-093" | material: layers "75 % 2669794085 100" ("75 % 2669794085" 100.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          1 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Cadre vertical 18" | names: "MOB-0055" | material: "Sans Trame" | property sets: AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre coulissante 2 vantaux 18" | names: "Fen-094" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "15 % 196800 230" | FLOOR | names: "Dalle-028" | material: layers "15 % 196800 230" ("15 % 196800" 230.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCSLAB | type IFCSLABTYPE "15 % 196800 180" | FLOOR | names: "Dalle-028" | material: layers "15 % 196800 180" ("15 % 196800" 180.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Struct. - B.A. coulé 200 x 200" | object type "Struct. - B.A. coulé 200 x 200" | names: "Pou-036" | material: "Struct. - B.A. coulé" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          13 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "100 % 2668484876 80" | names: "Mur-082", "Mur-094", "Mur-093" | material: layers "100 % 2668484876 80" ("100 % 2668484876" 80.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre double 18" | names: "Fen-095", "Fen-094" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCWINDOW | type IFCWINDOWSTYLE "Fenêtre double 18" | names: "Fen-094" | material: materials ("Sans Trame", "Lame d'air", "Sans Trame", "Sans Trame", "Sans Trame", "Isolation polystyrène", "Sans Trame", "Sans Trame", "Sans Trame", "Sans Trame", "Lame d'air", "Sans Trame", "_U") | property sets: Pset_WindowCommon, Pset_FireRatingProperties, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, AC_Pset_RenovationAndPhasing
          1 x IFCSLAB | type IFCSLABTYPE "75 % 2669794085 41" | ROOF | names: "Toit-24" | material: layers "75 % 2669794085 40.8654" ("75 % 2669794085" 40.8653739891) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
      IFCBUILDINGSTOREY "R+2 / 87.25 ngf" | elevation 6610.
        contains 323 elements
          141 x IFCCOLUMN | type IFCCOLUMNTYPE "25 % 2670121569 100 x 50" | object type "25 % 2670121569 100 x 50" | names: "Pot-039" | material: "25 % 2670121569" | property sets: AC_Pset_RenovationAndPhasing, Pset_ColumnCommon
          1 x IFCBEAM | type IFCBEAMTYPE "Bois 45 2682958634 50 x 0" | object type "Bois 45 2682958634 50 x 0" | names: "Pou-034" | material: "Bois 45 2682958634" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          3 x IFCSLAB | type IFCSLABTYPE "15 % 196800 200" | FLOOR | names: "Dalle-028" | material: layers "15 % 196800 200" ("15 % 196800" 200.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          4 x IFCBEAM | type IFCBEAMTYPE "Bois 45 2682958634 50 x 105" | object type "Bois 45 2682958634 50 x 105" | names: "Pou-034" | material: "Bois 45 2682958634" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          144 x IFCFURNISHINGELEMENT | type IFCFURNISHINGELEMENTTYPE "Arbalétrier 18" | names: "MOB-0061" | material: "Sans Trame" | property sets: AC_Pset_RenovationAndPhasing
          2 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "15 % 196800 180" | names: "Mur-089" | material: layers "15 % 196800 180" ("15 % 196800" 180.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          2 x IFCSLAB | type IFCSLABTYPE "75 % 2669794085 80" | ROOF | names: "Toit-23" | material: layers "75 % 2669794085 80" ("75 % 2669794085" 80.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
          6 x IFCWALLSTANDARDCASE | type IFCWALLTYPE "15 % 196800 30" | names: "Mur-093", "Mur-094", "Mur-095" | material: layers "15 % 196800 30" ("15 % 196800" 30.) | property sets: AC_Pset_RenovationAndPhasing, Pset_WallCommon
          3 x IFCBEAM | type IFCBEAMTYPE "Bois 45 2682958634 50 x 108" | object type "Bois 45 2682958634 50 x 108" | names: "Pou-034" | material: "Bois 45 2682958634" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          14 x IFCBEAM | type IFCBEAMTYPE "Bois 45 2682958634 50 x 100" | object type "Bois 45 2682958634 50 x 100" | names: "Pou-034" | material: "Bois 45 2682958634" | property sets: AC_Pset_RenovationAndPhasing, Pset_BeamCommon
          3 x IFCSLAB | type IFCSLABTYPE "15 % 196800 40" | FLOOR | names: "Dalle-029" | material: layers "15 % 196800 40" ("15 % 196800" 40.) | property sets: AC_Pset_RenovationAndPhasing, Pset_SlabCommon
      IFCBUILDINGSTOREY "PLAN MASSE / 2D" | elevation 102610.

Types
  IFCSLABTYPE "15 % 196800 600" | 5 occurrences
  IFCCOLUMNTYPE "25 % 2670121569 D50" | 1 occurrence
  IFCSLABTYPE "75 % 2669794085 1380" | 1 occurrence
  IFCCOLUMNTYPE "25 % 2670121569 D30" | 44 occurrences
  IFCWALLTYPE "75 % 2034597177 300" | 7 occurrences
  IFCWALLTYPE "15 % 196800 200" | 21 occurrences
  IFCWALLTYPE "HACHURE MANQUANTE 269029580 450" | 8 occurrences
  IFCWALLTYPE "75 % 2034597177 270" | 2 occurrences
  IFCWALLTYPE "75 % 2034597177 200" | 3 occurrences
  IFCWALLTYPE "75 % 2669925280 200" | 1 occurrence
  IFCWINDOWSTYLE "Fenêtre 18" | SINGLE_PANEL | 3 occurrences | property sets: Propriétés Doublure Fenêtre, Propriétés Panneau Fenêtre - Panneau1
  IFCCOLUMNTYPE "25 % 2670121569 D200" | 2 occurrences
  IFCFURNISHINGELEMENTTYPE "Tube rampe 18" | 2 occurrences
  IFCWALLTYPE "75 % 2669925280 100" | 4 occurrences
  IFCWALLTYPE "100 % 2668484876 80" | 15 occurrences
  IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 150" | 18 occurrences
  IFCWINDOWSTYLE "Fenêtre 18" | SINGLE_PANEL | 1 occurrence | property sets: Propriétés Doublure Fenêtre, Propriétés Panneau Fenêtre - Panneau1
  IFCWALLTYPE "100 % 2668484876 200" | 1 occurrence
  IFCSLABTYPE "15 % 196800 230" | 2 occurrences
  IFCSLABTYPE "100 % 2668484876 70" | 2 occurrences
  IFCBEAMTYPE "Bois 45 2682958634 200 x 200" | 1 occurrence
  IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 20" | 3 occurrences
  IFCWALLTYPE "100 % 2668484876 340" | 1 occurrence
  IFCWINDOWSTYLE "Fenêtre 18" | SINGLE_PANEL | 3 occurrences | property sets: Propriétés Doublure Fenêtre, Propriétés Panneau Fenêtre - Panneau1
  IFCBEAMTYPE "Bois 45 2682958634 200 x 520" | 1 occurrence
  IFCSLABTYPE "15 % 196800 40" | 4 occurrences
  IFCSLABTYPE "100 % 2668484876 503" | 1 occurrence
  IFCSLABTYPE "100 % 2668484876 930" | 1 occurrence
  IFCSLABTYPE "100 % 2668484876 645" | 1 occurrence
  IFCSLABTYPE "100 % 2668484876 788" | 1 occurrence
  IFCWALLTYPE "100 % 2668484876 20" | 1 occurrence
  IFCWALLTYPE "0 - HACHURE ISOLANT 309885812 60" | 1 occurrence
  IFCFURNISHINGELEMENTTYPE "Poutre acier universel 18" | 2 occurrences
  IFCFURNISHINGELEMENTTYPE "Cadre main cour 18" | 3 occurrences
  IFCWALLTYPE "100 % 859257570 200" | 1 occurrence
  IFCWINDOWSTYLE "Ouverture fenêtre rectangulaire 18" | USERDEFINED | 3 occurrences
  IFCWALLTYPE "75 % 2669794085 100" | 4 occurrences
  IFCFURNISHINGELEMENTTYPE "Cadre vertical 18" | 1 occurrence
  IFCWINDOWSTYLE "Fenêtre coulissante 2 vantaux 18" | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: Propriétés Doublure Fenêtre, Propriétés Panneau Fenêtre - Panneau1, Propriétés Panneau Fenêtre - Panneau2
  IFCSLABTYPE "15 % 196800 180" | 1 occurrence
  IFCBEAMTYPE "Struct. - B.A. coulé 200 x 200" | 1 occurrence
  IFCWINDOWSTYLE "Fenêtre double 18" | DOUBLE_PANEL_VERTICAL | 2 occurrences | property sets: Propriétés Doublure Fenêtre, Propriétés Panneau Fenêtre - Panneau1, Propriétés Panneau Fenêtre - Panneau2
  IFCWINDOWSTYLE "Fenêtre double 18" | DOUBLE_PANEL_VERTICAL | 1 occurrence | property sets: Propriétés Doublure Fenêtre, Propriétés Panneau Fenêtre - Panneau1, Propriétés Panneau Fenêtre - Panneau2
  IFCSLABTYPE "75 % 2669794085 41" | 1 occurrence
  IFCCOLUMNTYPE "25 % 2670121569 100 x 50" | 141 occurrences
  IFCBEAMTYPE "Bois 45 2682958634 50 x 0" | 1 occurrence
  IFCSLABTYPE "15 % 196800 200" | 3 occurrences
  IFCBEAMTYPE "Bois 45 2682958634 50 x 105" | 4 occurrences
  IFCFURNISHINGELEMENTTYPE "Arbalétrier 18" | 144 occurrences
  IFCWALLTYPE "15 % 196800 180" | 2 occurrences
  IFCSLABTYPE "75 % 2669794085 80" | 2 occurrences
  IFCWALLTYPE "15 % 196800 30" | 6 occurrences
  IFCBEAMTYPE "Bois 45 2682958634 50 x 108" | 3 occurrences
  IFCBEAMTYPE "Bois 45 2682958634 50 x 100" | 14 occurrences

Property sets
  AC_Pset_RenovationAndPhasing | properties | on 505 objects (188 IFCCOLUMN, 152 IFCFURNISHINGELEMENT, 99 IFCWALLSTANDARDCASE, 25 IFCBEAM)
    Renovation Status = "Existing" (IFCLABEL)
  Pset_SlabCommon | properties | on 21 objects (21 IFCSLAB)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_SlabCommon | properties | on 4 objects (4 IFCSLAB)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = FALSE (IFCBOOLEAN)
  Pset_ColumnCommon | properties | on 141 objects (141 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "25 % 2670121569 100 x 50" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 44 objects (44 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "25 % 2670121569 D30" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 2 objects (2 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "25 % 2670121569 D200" (IFCIDENTIFIER)
  Pset_ColumnCommon | properties | on 1 object (1 IFCCOLUMN)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "25 % 2670121569 D50" (IFCIDENTIFIER)
  Pset_WallCommon | properties | on 99 objects (99 IFCWALLSTANDARDCASE)
    IsExternal = TRUE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
  Pset_StairCommon | properties | on 2 objects (2 IFCSTAIR)
    IsExternal = FALSE (IFCBOOLEAN)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
  Pset_WindowCommon | properties | on 3 objects (3 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.21499996094 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0. (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 0.693672424406 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.7 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 2.415 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 3.46499996651 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon | properties | on 1 object (1 IFCWINDOW)
    AcousticRating = "" (IFCLABEL)
    FireRating = "" (IFCLABEL)
    GlazingAreaFraction = 1.785 (IFCPOSITIVERATIOMEASURE)
    ThermalTransmittance = 0. (IFCTHERMALTRANSMITTANCEMEASURE)
  Pset_WindowCommon: 2 more contents on 2 objects not shown
  Pset_FireRatingProperties | properties | on 14 objects (14 IFCWINDOW)
    FireResistanceRating = "" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 11 objects (11 IFCWINDOW)
    SerialNumber = "" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 11 objects (11 IFCWINDOW)
    Manufacturer = "" (IFCLABEL)
    ProductionYear = "" (IFCLABEL)
  Pset_BeamCommon | properties | on 14 objects (14 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Bois 45 2682958634 50 x 100" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 4 objects (4 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Bois 45 2682958634 50 x 105" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 3 objects (3 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Bois 45 2682958634 50 x 108" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Bois 45 2682958634 200 x 200" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Bois 45 2682958634 200 x 520" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Struct. - B.A. coulé 200 x 200" (IFCIDENTIFIER)
  Pset_BeamCommon | properties | on 1 object (1 IFCBEAM)
    IsExternal = FALSE (IFCBOOLEAN)
    LoadBearing = TRUE (IFCBOOLEAN)
    Reference = "Bois 45 2682958634 50 x 0" (IFCIDENTIFIER)
  Propriétés Doublure Fenêtre | predefined | on 6 type objects
  Propriétés Panneau Fenêtre - Panneau1 | predefined | on 6 type objects
  Propriétés Panneau Fenêtre - Panneau2 | predefined | on 3 type objects